IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2019-09-10T23:12:26"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternate UI 20.0.0.377"
Application: "Autodesk Revit 2020 (ENG)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENG)"

People and organizations
  Person "lorenaluedy" of Organization (no name given)
  Owner history of Person "lorenaluedy" of Organization (no name given) | application "Autodesk Revit 2020 (ENG)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENG)" | change NOCHANGE | created 1566409656 (2019-08-21T17:47:36Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Nome do projeto" | phase "Status do projeto"
  IFCSITE "Default" | latitude 36° 31′ 6.893005″ | longitude -4° 53′ 3.947753″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Foundation" | long name "Foundation" | object type "Level:Cabeça de 8 mm" | elevation -0.3
        contains 2 elements
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Wall" | object type "Basic Wall:Wall" | names: "Basic Wall:Wall:287588", "Basic Wall:Wall:287668" | material: layers "Basic Wall:Wall" ("Brick, Common" 0.11) | property sets: BaseQuantities, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Cabeça de 8 mm" | elevation 0.
        contains 1 element
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Land" | object type "Floor:Land" | FLOOR | names: "Floor:Land:287333" | material: layers "Floor:Land" ("Land" 0.5) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, BaseQuantities

Types
  IFCWALLTYPE "Basic Wall:Wall" | STANDARD | 2 occurrences | material: layers "Basic Wall:Wall" ("Brick, Common" 0.11) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Floor:Land" | FLOOR | 1 occurrence | material: layers "Floor:Land" ("Land" 0.5) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon

Property sets
  Pset_ElementShading | properties | on 3 objects (2 IFCWALLSTANDARDCASE, 1 IFCSLAB) | on 2 type objects
    Roughness = 0.9144 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ProductRequirements | properties | on 2 objects (2 IFCWALLSTANDARDCASE) | on 1 type object
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Category = "Floors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Foundation" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 0" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Wall" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Land" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Land" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Land" (IFCIDENTIFIER)
    ThermalTransmittance = 1.674 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Land" (IFCIDENTIFIER)
    ThermalTransmittance = 1.674 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 9. [SQUARE_METRE]
    GrossVolume = 4.5 [CUBIC_METRE]
    NetArea = 24. [SQUARE_METRE]
    NetVolume = 4.5 [CUBIC_METRE]
    Perimeter = 12. [METRE]
    Width = 0.5 [METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.16445 [SQUARE_METRE]
    Height = 1.8 [METRE]
    Length = 1.495 [METRE]
    NetSideArea = 2.691 [SQUARE_METRE]
    NetSideArea = 2.691 [SQUARE_METRE]
    NetVolume = 0.29601 [CUBIC_METRE]
    NetVolume = 0.29601 [CUBIC_METRE]
    Width = 0.11 [METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.0978999999999999 [SQUARE_METRE]
    Height = 1.8 [METRE]
    Length = 0.89 [METRE]
    NetSideArea = 1.602 [SQUARE_METRE]
    NetSideArea = 1.602 [SQUARE_METRE]
    NetVolume = 0.17622 [CUBIC_METRE]
    NetVolume = 0.17622 [CUBIC_METRE]
    Width = 0.11 [METRE]
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Wall" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall" (IFCIDENTIFIER)
    ThermalTransmittance = 4.90909090909091 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Wall" (IFCIDENTIFIER)
    ThermalTransmittance = 4.90909090909091 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Foundation" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 0" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 2 (IFCINTEGER)

Other addresses and roles
  2 x postal address: "Insira aqui o endereço", "Calle Carlomagno", "1", "29601", "Marbella (Málaga)", "Espanha"